nhb100
#オートマットメッセージの目次
01,A01 No or Low Battery Voltage Error
02,A05 Wrong Tape Code or BAUD Rate Error
03,A07 IC Memory Error  
04,A08 Memory is Full or Design Memory Read Error 
05,A11 No PC or Peripheral Device Connected Error
06,A20 Memory Slot Empty 
07,A21 All Memory Slots are Empty
08,A24 No More Color Change Codes Found
09,A26 Sock Frame Origin Not Set
10,A27 No More Function Codes Found
11,A28 Calculating Please Wait
12,A29 Memory is Full
13,A30 Disk Not Mounted
14,A31 Floppy Write Protected Error
15,A32 Floppy Disk Read/Write Error
16,A33 Floppy File Full Error
17,A34 Too Many Color Changes in Design
18,A35 Spectacle Frame Error
19,A36 Applique Error
20,A37 USB Memory Device is Full
21,A38 No USB Memory Device Inserted
22,A39 USB Read/Write Error
23,A40 Network Error
24,A41 Design Data Reading Error
